| **Field Name** | **Description** | **Value** |
| --- | --- | --- |
| Section ID | Numerical identifier of pavement section | Number (no decimal) |
| Highway | Highway number | Text |
| Direction | Travelling direction in which the pavement condition data is collected. Generally, surveys are conducted in one direction only for undivided highways. | Text  Options:  E – East  W – West  N – North  S - South |
| LHRS | Location reference based on Linear Highway Reference System | Number (no decimal) |
| Offset | Location reference measured as the distance away from the LHRS | Number (with decimal) |
| From\_Distance | Start chainage in kilometre (km) of the reporting interval | Number (with decimal) |
| To\_Distance | End chainage in kilometre (km) of the reporting interval | Number (with decimal) |
| PCI | Overall Pavement Condition Index of reported pavement section | Number (with decimal) |
| DMI | Average Distress Manifestation Index of the pavement surface within the reporting interval | Number (with decimal) |
| IRI | Average International Roughness Index (m/km) of the pavement surface within the reporting interval | Number (with decimal) |
| Pave\_Type | One of the four pavement material types.  AC – Asphalt Concrete  PC – Portland Cement Concrete  COM – AC/PC Composite  ST – Surface-treated | Text  Options:  AC – Asphalt Concrete  PC – Portland Cement Concrete  COM – AC/PC Composite  ST – Surface-treated |
| Latitude | Latitude of the GPS coordinates of the starting point of the reporting interval, in N/W degree format | Number (with decimal) |
| Longitude | Longitude of the GPS coordinates of the starting point of the reporting interval, in N/W degree format | Number (with decimal) |
| Pavement\_Section\_From | Landmark description of starting point of the evaluated pavement section. Blank cells in the column indicate the evaluation is within the same pavement section. | Text |
| Pavement\_Section\_To | The landmark description of ending point of the evaluated pavement section. | Text |
| Function Class | One of the four function classes of the roadway:  FWY – Freeway  ART – Arterial Highway  COL – Collector  LOC – Local Road | Text  Options:  FWY – Freeway  ART – Arterial  COL – Collector  LOC – Local Road |